**The Relationship between Steel Plate Depth and Printing**

1. **Shallow plate is better for fine/thin lines. Deep plate is better for thick lines.**
2. **Use shallow plate if the printed object surface is smooth; Use deeper plate when the surface is etching and ink-absorbing.**
3. **Use shallow plate when printing dark ink on light object; Use deeper plate when printing light ink on dark object.**